{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":3,"rows_kept":16,"merged":[[0,0,0,2]],"flags":["formulas_cached_only"]}
["思埃玛智能科技伺服压机报警说明"]
["报警提示","注解","处置方式"]
["扭矩限制","伺服运行时扭矩超过设定的伺服内部限制扭矩","1.在触摸屏上参数设置界面“伺服出力”数值加大。2.若按以操作后还报警提示此内容，者可能丝杠损坏或机械结构卡住。"]
["NG↓","在检测位置起点和检测位置终点区间内\n当前压力＜检测下限压力    过松NG↓报警","1.在触摸屏参数设置界面“检测”中“下限（kg）”数值减小。\n2.或在触摸屏参数设置界面“检测”中“起点（mm）”数值加大。"]
["NG↑","在检测位置起点和检测位置终点区间内\n当前压力＞检测上限压力    过紧NG↑报警","1.在触摸屏参数设置界面“检测”中“上限（kg）”数值加大。\n2.或在触摸屏参数设置界面“检测”中“终点（mm）”数值减小。"]
["行程未到返回压力到达","压力到达设定返回压力\n但检测位置1起点＞实际压力到达时所在位置 行程未到报警（压力到达行程未到）","1.在触摸屏参数设置界面“检测”“位置设定1”中“起点（mm）”数值减小。\n2.或在触摸屏参数设置界面“返回压力”数值加大。"]
["超出行程返回压力未到","检测位置1终点＜实际压力到达时所在位置（或超出检测位置1终点时都还未到达返回压力） 超出行程报警（压力到达超出行程）","1.在触摸屏参数设置界面“检测”“位置设定1”中“终点（mm）”数值加大。\n2.或在触摸屏参数设置界面“返回压力”数值减小。"]
["压力未到","到精压段位置压力都还未到达设定返回压力","1.在触摸屏参数设置界面“精压段”中“位置（mm）”数值加大。\n2.或在触摸屏参数设置界面“返回压力”数值减小。"]
["超出系统最大压力","产生了超出系统设定最大压力","1.按下急停按钮，在触摸屏主界面点击报警复位按钮，在触摸屏主界面点击复位按钮。\n2.若按以操作后还报警提示此内容，请重启设备。"]
["伺服故障","具体原因看伺服报警代码","1.报警复位。\n2.若按以操作后还报警提示此内容，请重启设备。"]
["伺服缸下限位","压杆下行距离过长抵至下限位开关","1.在触摸屏手动界面点击慢速上升一段距离使压杆置于中间位置。\n2.若按以操作后还报警提示此内容，请重启设备。"]
["伺服缸上限位","压杆上行距离过长抵至上限位开关","1.在触摸屏手动界面点击慢速下降一段距离使压杆置于中间位置。\n2.若按以操作后还报警提示此内容，请重启设备。"]
["急停按钮被按下","急停按钮被按下","1.排除危险，旋转提起急停按钮。"]
["光栅被遮挡","有物体遮挡住了对射光栅","1.排除危险，移开遮挡住对射光栅的物体。"]
["无报警但经常出现位置不准","在压力模式下，以压力为主要运行判断，位置作为公差结果判断。","1.标准伺服压机采用的是压力传感器实时采集对比压力做出判断运行动作。长期使用建议采用柔性压装。2.若为定制型伺服转矩限制款则不受此限制，但会丧失对位置的精准控制。"]
[null,"运行时还会伴有异响，机械原因导致","1.长期使用或经常撞击可能使减速机、锁紧螺丝、锁紧螺母松动。锁紧即可。\n2.长期使用或经常撞击可能会导致内部丝杆与丝母产生间隙严重者可能发生形变。系此为人为损坏我司可能会收取部分费用。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}